                        3Com (R) Corporation
                     EtherDisk (R) Diskette for
                   The EtherLink 10 ISA NIC Family
                 MS LAN Manager Installation Notes


Microsoft LAN Manager Versions 2.0, 2.1, and 2.2
------------------------------------------------
The EtherDisk #2 diskette contains a subdirectory structure and files that
make it an OEM import disk for the LAN Manager installer.  Use the import
function of the LAN Manager installer to capture the NDIS driver from the
EtherDisk diskette.  Be sure to save the new configuration before exiting
the installer.


DOS Installation with LAN Manager 2.2
-------------------------------------
The following describes the procedure for importing the driver during
installation of LAN Manager 2.2 for DOS.

1.  Begin the MS-DOS LAN Manager installation by inserting the MS-DOS
    Setup diskette and typing:

    A:SETUP

2.  After reading the Microsoft Drivers 1 diskette, a window is displayed
    showing available network NIC drivers.  In this window choose the
    following function:

    Select Other Driver         (Alt-D)

3.  When prompted to insert your network driver diskette, insert the
    EtherDisk #2 diskette.

4.  After the driver is imported from the EtherDisk diskette, a box will
    be displayed showing the driver.  Select the EtherLink 10 ISA Family
    driver.

5.  Continue with the remainder of the installation by next selecting a
    protocol to use with the EtherLink 10 ISA Family driver.


                 (%VER LANMAN.TXT - MS LAN Manager v6.1a)


